{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Eficiencia-termicas","Fact Emision","Equivalencia"],"not_rendered":{"charts":0,"images":3,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Eficiencia-termicas","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Fact Emision","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Equivalencia","index":2,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Cantidad","De",null,"Cantidad","A",null,"Prefijo","Multiplicador","Abreviatura"]
[null,1,"Julio","=",{"$f":"CONVERT(B4,\"J\",\"kWh\")","v":2.7777777777777776E-7},"kWh",null,"exa",1E+18,"\"E\""]
[null,1,"GJ","=",{"$f":"CONVERT(B5,\"GJ\",\"BTU\")","v":947817.12031331717},"BTU"]
[null,1,"MWh","=",{"$f":"CONVERT(B6,\"MWh\",\"GJ\")","v":3.6},"GJ",null,"peta",1000000000000000,"\"P\""]
[null,1,"MWh","=",{"$f":"CONVERT(B7,\"MWh\",\"MJ\")","v":3600},"MJ",null,"tera",1000000000000,"\"T\""]
[null,1,"BTU","=",{"$f":"CONVERT(B8,\"BTU\",\"J\")","v":1055.05585262},"Julios",null,"giga",1000000000,"\"G\""]
[null,1,"BTU","=",{"$f":"CONVERT(B9,\"BTU\",\"kJ\")","v":1.05505585262},"KJ",null,"mega",1000000,"\"M\""]
[null,1,"BTU","=",{"$f":"CONVERT(B10,\"BTU\",\"kcal\")","v":0.25199576111111116},"kcal",null,"kilo",1000,"\"k\""]
[null,1,"cal","=",{"$f":"CONVERT(B11,\"cal\",\"J\")","v":4.1867999999999999},"Julios",null,"hecto",100,"\"h\""]
[null,1,"m","=",{"$f":"CONVERT(B12,\"m\",\"ft\")","v":3.2808398950131235},"pie",null,"deca",10,"\"e\""]
[null,1,"m3","=",{"$f":"E12^3","v":35.314666721488592},"pie3",null,"deci",0.1,"\"d\""]
[null,1,"kWh","=",{"$f":"CONVERT(B14,\"kWh\",\"btu\")","v":3412.1416331279415},"Btu",null,"centi",0.01,"\"c\""]
[null,1,"kWh","=",{"$f":"CONVERT(B15,\"kWh\",\"kcal\")","v":859.84522785898537},"kcal",null,"mili",1E-3,"\"m\""]
[null,1,"hp-hora","=",0.746,"kWh",null,"micro",9.9999999999999995E-7,"\"u\""]
[null,1,"hp-hora","=",2545,"BTU",null,"nano",1.0000000000000001E-9,"\"n\""]
[{"$nulls":7},"pico",9.9999999999999998E-13,"\"p\""]
[null,"Eficiencia %","(en terminos de BTU)",null,{"$f":"E14/12000","v":0.28434513609399514},null,null,"femto",1.0000000000000001E-15,"\"f\""]
[null,"(un equipo con un Heat Rate = 12000 Btu/kWh)",{"$nulls":5},"atto",1.0000000000000001E-18,"\"a\""]
[null,"Eficiencia %","(en terminos de kCal)",null,{"$f":"E15/(12000*E10)","v":0.28434513609399509}]
[null,"(un equipo con un Heat Rate = 12000 Btu/kWh  =  3023.9594 kCal/kWh)"]
[]
[null,null,null,"1 pulgada (1\") = 2,54 cm"]
[null,null,null,"1 pie (1') = 30,48 cm"]
[null,null,null,"l libra (1 lb) = 0,4536 kg"]
[null,null,null,"2202,6 libras = 1 tonelada (1 ton)"]
[null,null,null,"1 lb/pulg² = 6,895 kPa"]
[null,null,null,"1 pulg de mercurio (Hg) = 3,386 kPa"]
[null,null,null,"1 pulg agua = 249 Pa"]
[null,null,null,"1 atmósfera (1 atm) = 101,325 kPa"]
[null,null,null,"1 BTU (British Thermal Unit) = 1,054 kJ"]
[null,null,null,"1 hph = 2,685 MJ"]
[null,null,null,"1 hp = 746 W"]
[null,null,null,"1,34 hp = 1 kW"]